# File to provide fine control on some Mirone modules.
# Control options are indicated by the MIR_XXX keyword.
# Specific options follow on the rest of the line. Comment (#) each that you don't want to use

# For gmtedit the general usage is:
# -Vvar1,var2,var3:varI+slotI[/varI+slotI[/varI+slotI]] 
# Where var1,var2,var3 is the name of any of the variables in the .nc file PLUS 'vel' for velocity
# The varI+slotI form will plot (add) the varI (again, one of the .nc vars) to the slot I (1:3) axes 
# Next will put Total field on first axes, CM4 anomaly on second and bathymetry on third
#MIR_GMTEDIT -Vfaa,cm4_dc,depth
#MIR_GMTEDIT -Vvel,mtf1,depth
#MIR_GMTEDIT -Vlon,lat,vel
#MIR_GMTEDIT -Vvel,mtf1,anom_cm4:mag+3

# Activate MGG (.nc) tracks fishing inside rectangles (comment (#) if not wanted)
# Second field contains any or a combination of the G M T letters that stand for Grav Mat Topo.
# Example M use mgg files that contain Magnetic data, GMT use files that have at least one of G, M or T
MIR_MGG GMT

# Activate ROI Microleveling
MIR_MICROLEV

# Activate the option to display COEs as circles with uicontexts
MIR_COEs C:\a1\mgd77\COEs_17_linear.dat best_cm4

# Mag synthetic profiles params
MIR_MAGPROF DEC -21.2
MIR_MAGPROF INC 78.2
#MIR_MAGPROF SPEED 2.3
#MIR_MAGPROF SPREADIR 99.0
MIR_MAGPROF CONTAMIN 1.0
MIR_MAGPROF BAT C:\j\cd_grids\w_bat_atl.grd
# Third column holds anomaly age at its center (1.85), window half-width (1.1) and pecentage of stretch/shrink (15)
MIR_MAGPROF ISOC 1.86_0.6_15
MIR_MAGPROF ISOC 3.08_1.3_15
MIR_MAGPROF ISOC 4.66_1.4_15
MIR_MAGPROF ISOC 6.17_1.0_15
MIR_MAGPROF ISOC 7.54_1.0_15
MIR_MAGPROF ISOC 8.85_0.8_15
MIR_MAGPROF ISOC 10.33_1.4_15

# Custom CPT files that will show up in 'Thematic' of the Color Palettes tool
# The syntax is MIR_CPT 'palete_name' full_file_path
#MIR_CPT zzz C:\a1\pathfinder\zzz.cpt

# Outward displacement (for Euler poles computation). If commented OD is not applied.
#MIR_OD C:\SVN\mironeWC\continents\OD_simples.dat
#MIR_OD C:\SVN\mironeWC\continents\out_displacement.dat

# File with case selection and the EXACT arguments to run one of the main functions in aquaPlugin
#MIR_AQUAPLUG C:\SVN\mironeWC\data\example_data\aquaplug_CASE10_sc.txt 

# Activate the option to display the GMT database polygons ID inside a ROI rectangle
MIR_GMT_DB_IDS

# Activate the options to add custom menus with directories where to look for specific files
MIR_CUSTOM_MENU Geography,GRIDS/SRTM+,C:\j\cd_grids\SRTM+
MIR_CUSTOM_MENU Geography,GRIDS/cd_grids,C:\j\cd_grids
MIR_CUSTOM_MENU Geography,GRIDS/mag_grids,C:\j\cd_grids\mag
MIR_CUSTOM_MENU Geography,Seafloor/geomorphic,C:\SVN\mironeWC\data\seafloor_geomorphic
MIR_CUSTOM_MENU CustomIsoc,AF-NA,C:\SVN\mironeWC\data,isochrons_AF_NA.dat,Isochron
MIR_CUSTOM_MENU CustomIsoc,IB-NA,C:\SVN\mironeWC\data,isochrons_IB_NA.dat,Isochron
MIR_CUSTOM_MENU CustomIsoc,EU-NA,C:\SVN\mironeWC\data,isochrons_EU_NA.dat,Isochron
MIR_CUSTOM_MENU CustomIsoc,EU-GR,C:\SVN\mironeWC\data,isochrons_EU_GR.dat,Isochron
MIR_CUSTOM_MENU CustomIsoc,RO-NA,C:\SVN\mironeWC\data,isochrons_RO_NA.dat,Isochron
MIR_CUSTOM_MENU CustomIsoc,JM-EU,C:\SVN\mironeWC\data,isochrons_JM_EU.dat,Isochron
MIR_CUSTOM_MENU CustomIsoc,EU-MO,C:\SVN\mironeWC\data,isochrons_EU_MO.dat,Isochron
MIR_CUSTOM_MENU CustomIsoc,EU-LO,C:\SVN\mironeWC\data,isochrons_EU_LO.dat,Isochron
MIR_CUSTOM_MENU CustomIsoc,GR-NA,C:\SVN\mironeWC\data,isochrons_GR_NA.dat,Isochron
MIR_CUSTOM_MENU CustomIsoc,KT-NA,C:\SVN\mironeWC\data,isochrons_KT_NA.dat,Isochron
MIR_CUSTOM_MENU MagGrav,MAG8_RTP,C:\j\cd_grids,mag8_rtp.grd

# Activate the option to associate a GMT custom symbol to a line (rectangle) object
MIR_GMT_SYMBOL

# Activate the option to compute a gravity anomaly inside the rectangle object
MIR_GRAVITY

# Finite poles to associate to isochrons. Used by the line's uicontext option "Update poles in headers"
MIR_POLES_FOR_ISOC C:\SVN\mironeWC\data\isocs\polos_para_idades_EU_NA.dat
